4.3. WINDOWS OF XGUI 55

4.3.9 Print Panel The print panel handles the Postscript output. A 2D-display can be associated with the printer. All setup options and values of this display will be printed. Color and encapsulated Postscript are also supported. The output device is either a printer or a file. If the output device is a printer, a ’.ps’-file is generated and spooled in the /tmp directory. It has a unique name starting with the prefix ‘snns’. The directory must be writable. When xgui terminates normally, all SNNS spool files are deleted.

Figure 4.19: Printer panel

The following fields can be set in the Printer Panel, which is shown in figure 4.19.

1. File Name resp. Command Line:

If the output device is a file: the filename.

If the output device is a printer: the command line to start the printer. The filename in the command line has to be ’$1’.

2. Destination: Selects the output device. Toggles the above input line between File Name and Command Line.

3. Paper: Selects the paper format.

4. Orientation: Sets the orientation of the display on the paper. Can be ’portrait’ or ’landscape’.

5. Border (mm): Sets the size of the horizontal and vertical borders on the sheet in millimeters.

6. AutoScale: Scales the network to the largest size possible on the paper. 7. Aspect: If on, scaling in X and Y direction is done uniformly. 8. X-Scale: Scale factor in X direction. Valid only if AutoScale is ’OFF’. 9. Y-Scale: Scale factor in Y direction. Valid only if AutoScale is ’OFF’.

DONE : Cancels the printing and closes the panel.
PRINT : Starts printing.